______________________________________________________________________________

ReadMe.txt
______________________________________________________________________________

Copyright (C) 2007 Oxford Semiconductor Ltd.

Driver for legacy mode UARTs of PCIe952 family devices.

____________________________
Installation
____________________________

1. Install Windows CE 5.00 Platform Builder (PB) to a development PC and note
   the WINCEROOT i.e. the path where the CE5.0 is installed.

2. Execute the batch file "CopyDriverToWiunCERoot.bat" which will prompt the 
   user to enter the WINCEROOT. The batch file will then copy all the driver
   files to the WINCEROOT. The follow directory structure or similar shall be seen:
   
	C:\WINCE500\OXSEMI
	               |------UARTS
	               |        |
	               |        |-----....
	               |        |-----PCIE952_UART
	               |        |-----INC
	               |        \-----....
	               |
	               \------....

3. Start Platform Builder and create a platform.

4. Click “File->Manage Catalog Features” to start “Manage Catalog Features” dialog

5. Click “Import…” button to start “Import Catalog Features” dialog and import 
   cec files of “pcie952_uart.cec” in the subdirectory of “\uarts\pcie952_uart\"

6. Add "COM16550" feature to the platform by right-click on its logo and choose
   “Add to Platform”

7. Add "pcie952_uart" feature to the platform by right-click on its logo and
   click on “Add to Platform”

8. Start platform build process by clicking “Build OS->Build and Sysg" or simply
   remake the OS image by "Build OS->Make Run-Time Image" if a image is existing
________________________________________________________________________________

                                 End of ReadMe
________________________________________________________________________________
